Document No. EX##-TDW0017
March 1, 2019
Product Development Div.5, SMC Corporation


Dear users of the serial transmission unit, EX260-SIL1,
Please be informed of notes of the setup file, IODD file.
IO-Link data transmission rate and process data size can be set by the
switch.
The IODD file is different for each settings.
Please use an appropriate IODD file for each settings.


1.SMC-EX260-SIL1_04_3-yyyymmdd-IODD1.1
- Data Transmission rate : COM3(230.4kbps)
- Process data size      : 0 byte input/4 bytes output

2.SMC-EX260-SIL1_04_2-yyyymmdd-IODD1.1
- Data Transmission rate : COM2(38.4kbps)
- Process data size      : 0 byte input/4 bytes output

3.SMC-EX260-SIL1_24_3-yyyymmdd-IODD1.1
- Data Transmission rate : COM3(230.4kbps)
- Process data size      : 2 bytes input/4 bytes output

4.SMC-EX260-SIL1_24_2-yyyymmdd-IODD1.1
- Data Transmission rate : COM2(38.4kbps)
- Process data size      : 2 bytes input/4 bytes output
